**SECTION 11 16 16**

**SAFES**

**PART 1 GENERAL**

1. RELATED DOCUMENTS
	1. Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division‑1 specification section, apply to work of this section
2. SECTION INCLUDES
	1. Drop safe
3. SUBMITTALS FOR REVIEW
	1. Section 01 33 00 – Submittals Procedures
	2. Product Data: Provide UL listing/rating, insurance ratings, dimensions, and anchorage/installation instructions.
	3. Provide the manufacturer's warranty information.

**PART 2 PRODUCTS**

1. COMPONENTS
	1. Safe with hopper emptying into the safe and these minimum requirements:
		1. 1-hour UL Fire Rating
		2. UL RSC Burglary Rating
		3. Inside dimensions 22" H x 18" W x 16" D
		4. Hopper with steel frame capable of handling a 3½" x 9" x 11½ “package
		5. Outer door UL listed group II Changeable dial combination lock
	2. The District will review request for approved equal.

**PART 3 EXECUTION**

1. EXAMINATION
	1. Verify existing site conditions.
2. INSTALLATION
	1. Install safe in accordance with manufacturer's instructions in the location shown on plans.
	2. Provide all material, accessories, and labor to complete the installation

END OF SECTION